| **VIDEO P6-1-ALL-RESHOOT Version 1** | | |
| --- | --- | --- |
| Cell | **Visuals** | **Audio** |
| 1 | **Video 1-2 replace screen capture from 0:46 – 1:00**  SCREEN CAPTURE:  P6-1-2-reshoot\_capture1.trec  (show "\" instead of "¥") | N/A |
| 2 | **Video 1-2 replace screen capture from 1:16 – 3:06**  SCREEN CAPTURE:  P6-1-2-reshoot\_capture2.trec  (show "\" instead of "¥") | N/A |
| 3 | **Video 1-3 replace audio and screen capture from 3:47 – 4:00**  SCREEN CAPTURE:  P6-1-3-reshoot\_capture1.trec | Modified text: **Replace audio from 3:47 – 4:00**  I'll double click that component, change its name to PWM, I'll change the period to 999 and the compare to 500 which will give me a 50% duty cycle because the counter will count from 0 to 999. |
| 4 | N/A – this cell and screen capture number 2 not used | N/A |
| 5 | **Video 1-3 replace screen capture from 5:19 – 5:32**  SCREEN CAPTURE:  P6-1-3-reshoot\_capture3.trec  (show program instead of build  and show debug target window) | Modified text (mostly new) – **Replaces audio from 5:19 to 5:32.**  Click the program button and it will build the application and program the device that I already have connected to the type-C port on my laptop. When you click on program, you may see a Select Debug Target window. If so, you need to select either the CM0 plus or the CM4 to specify which device's SWD interface to use since they can both connect to the debugger. It doesn't matter which one you choose since they both are able to program the flash with your project, but since it is more likely that you will want to debug the CM4 later, I'll choose that one. Then I click on "OK/Connect" and the device is programmed. |
| 6 | **Video 1-3 replace screen capture from 5:37 – 5:50**  SCREEN CAPTURE:  P6-1-3-reshoot\_capture4.trec  (show "\" instead of "¥") | N/A |
| 7 | **Video 1-3 replace screen capture from 7:58 – 8:02**  SCREEN CAPTURE:  P6-1-3-reshoot\_capture5.trec  (show program button) | N/A |
| 8 | **Video 1-3 at 8:24**  N/A | Modified text:  I'm gonna right click on the project name and select copy, then right click on the workspace name and select paste. |
| 9 | **Video 1-3 replace screen capture from 9:03 – 9:08**  SCREEN CAPTURE:  P6-1-3-reshoot\_capture6.trec  (show program instead of build) | N/A |
| 10 | **Video 1-4 replace screen capture from 0:58 - 1:10**  SCREEN CAPTURE:  P6-1-4-reshoot\_capture1.trec  (show "\" instead of "¥") | N/A |
| 11 | **Video 1-4 replace screen capture from 4:42 – 4:47**  SCREEN CAPTURE:  P6-1-4-reshoot\_capture2.trec  (show program button) | N/A |