| **VIDEO P6-2-4a-KillSwitch Version 2** | | |
| --- | --- | --- |
| Cell | **Visuals** | **Audio** |
| 1 |  | Welcome back to Cypress Academy, PSoC 6 101. In this video, I will show you how to add custom digital logic to our BLE-controlled robotic arm to safely stop the servos and bypass any UART or I2C commands. We will also use the RGB LED on the PSoC 6 Pioneer Board to show the kill-switch status. |
| 2 | VIDEO:  Can we get stock footage of a killer rampaging robot? I'm guessing using a scene from a Terminator movie isn't going to be allowed. | Why a kill switch in a BLE-controlled robotic arm you might ask? Well (1) because all robots should always have a kill switch - has anyone seen the Terminator movies? - and (2) because my son, bless his heart, is an avid engineer and tinkerer much like his dad and while working on the robotic arm assembly, he most certainly will be tinkering with the control interfaces and swinging the robot arm every which way. |
| 3 |  | All joking aside, the real reason for a kill switch is to remove the CPU from a safety critical decision. Our digital logic responds in nanoseconds, CPUs are much slower, microseconds or even more depending on what’s going on in your application. |
| 4 | TEXT ON SCREEN:  When Alan says: "that you can find here", show this link:  NEED TO KNOW WHAT ALAN HAS IN MIND FOR THIS LINK – UDB Editor? Is that the best introduction to UDBs? | So, we’re going to make a simple t-flip-flop controlled by an external switch on the PSoC 6 BLE Pioneer board. The t-flip-flop will be implemented in the digital logic in the PSoC 6, called the Universal Digital Block, or UDB for short. There’s a lot more documentation on this and entire video series on this that you can find here: <point>. |
| 5 | SCREEN CAPTURE:  P6-6-4a-KillSwitch\_capture1.trec | Let’s get started.  I’ll create a new project called “BasicKillSwitch”. For this project I want to use a button on the PSoC 6 BLE Pioneer board to act as the kill switch. When I enable the kill switch, I expect the red led to immediately turn on and blink. When I disable the kill switch, I expect to see a solid green LED indicating all is well.  To do this, I’ll drag and drop a t-flip-flop from the digital logic folder in the component catalog. Add a digital input pin component. Let’s rename that pin “SW” and set the drive mode to resistive pull-up on the general tab of the pin dialog. I’m doing that because the push button on the PSoC 6 BLE kit is active low.  Now, I’ll connect the switch to the t-flip-flop through an invertor to make the switch act on the falling edge. I also need a logic high for the t-input of the flip-flop. With this configuration, the output of the flip-flop will toggle each time the button is pressed. To enable a blinking LED, we’re going to need a PWM. So, I’ll drag and drop a PWM into my design and configure it. I’ll rename the PWM LEDBlink. I’ll set the period to 1,000 and compare value to 500. I need a clock to input to the PWM, so another drag and drop, configure and now we have a 1KHz clock.  Now I have two LEDs in this project, a RED LED and a Green LED. So, let’s grab two digital output pins and rename them RED and GREEN. One thing to note with the LEDs is that they are active low, zero is on.  Now for a little logic fun. When the t-flip-flop output is high, disabled, I want to turn the Green LED on. So, a simple inverter logic block will do the trick. Drag and drop, wire that up, and good. Now if the t-flip-flop is low, enabled, I want to blink the red LED, so we’ll use a digital multiplexer and the output of the t-flip-flop to select the channel to send to the LED. We’ll send the LEDBlink PWM output to the multiplexer input 0 and a logic high to the multiplexer input 1. So, when the t-flip-flop output is low then the PWM output is feeding the RED LED, making it blink.  Let’s not forget to assign the pins for the switch, the red LED and green LED to P0[4], P0[3], and P1[1]; respectively. |
| 6 | SCREEN CAPTURE:  P6-6-4a-KillSwitch\_capture2.trec | In main\_cm4 you just need to start the PWM by calling LEDBlink\_Start() |
| 7 | SCREEN CAPTURE:  P6-6-4a-KillSwitch\_capture3.trec  VIDEO:  Show person pressing the button and the LED switching from blinking red to solid on green. | And that’s it. Build, program and test…again, love those blinky leds! |
| 8 |  | In the next video I will integrate the kill switch into our main robot controller. |
| 9 | TEXT ON SCREEN:  Cypress Developer Community  community.cypress.com  VIDEO:  Show video of ARH email and twitter windows. | You can post your comments and questions in our PSoC 6 community or as always you are welcome to email me at alan\_hawse@cypress.com or tweet me at @askioexpert with your comments, suggestions, criticisms and questions. |